Technical Note
                        No. 370/1                page 1 of 1

       Subject:         Difference to german type for french certification

       Effectivity:     DG-600 all versions for export to france

       Accomplishment:  During production

       Instructions:    1. Installation of a trim weight box according to
                           drawing R 19 in the front seatshell at the
                           right hand side of the instrument console

                        2. Balancing the sailplane for a min. cockpit
                           load of max. 65 kg or max. 85 kg if the DG-600
                           is equipped with the optional fin battery
                           installation.

                        3. T-handle for the tow release according to
                           drawing R 77.

       Remarks:         This TN is only effective for Export to France

                                                                        

       Bruchsal 4, date 13.03.1989

       Author:

              Dipl. Ing. W. Dirks

       Type certification inspector:

              Dipl. Ing. (FH) A. Güntert